OMOJOLA TEMILOLUWA OLUWATOMISIN

17/ENG04/058

ELECTRICAL/ELECTRONICS ENGINEERING

ENG 281 ASSIGNMENT 4

commandwindow

clear

clc

A=[1 -2 -1 3; 2 3 0 1; 1 0 -4 -2; 0 -1 3 1]

eig(A)

A=

 1 -2 -1 3

 2 3 0 1

 1 0 -4 -2

 0 -1 3 1

ans =

 2.4323 + 2.2437i

 2.4323 - 2.2437i

 -1.9323 + 1.7651i

 -1.9323 - 1.7651i

This system is unstable, because; the eigenvalues are a combination of both positive and negative values.