1 The power factor of a synchronous motor is changed with a change in the excitation. When the excitation of the motor is increased, the power factor changes from lagging to unity and then to a leading power factor. This property of the motor is utilized to improve the power factor of the leads, having a low lagging power factor. Normally, when the motor is utilized in this way to improve the factor, the synchronous motor is run without any mechanical load. The excitation is adjusted in such a manner that it is at a leading power factor.

2 That means that the three phase current entering the stator winding has an angle difference with the voltage

The purpose of using synchronous motors is to use it in leading power factor By controlling the field current in the rotor

3 An over-excited synchronous motor has a leading power factor. This makes it useful for power factor correction of industrial loads. Because the synchronous motor act has a capacitor which is useful in power factor improvement. Hence a synchronous motor is over excited this improves the plant power factor and reduces the reactive current required from the grid.

4 A synchronous motor has better power factor as compared to that of an equivalent induction motor. This is mainly because

 A. synchronous motor has no slip

 B. stator supply is not required to produce magnetic field

C. mechanical load on the rotor remains constant

 D. synchronous motor has large airgap

5 Synchronous motors are used for the power factor correction Now, since the set up of the magnetic flux (which can be considered as the reactive power component) inside the motoris done by the dc excitation provided on the rotor terminals, the power factor can also be controlled by controlling this dc excitation.

6 A synchronous motor running on no-load with leading power factor-will act as synchronous condenser.

The same motor when operated with lagging power factor on no-load will draw a reactive current from the system depending upon the system voltage.

7 Like an induction machine, an under excited synchronous machine too will consume reactive power; a properly excited synchronous machine neither consumes nor produces reactive power; An over excited synchronous machine can produce reactive power.

8 Efficiency is higher than of an induction motor of the same output and voltage rating because there are neither losses related to slip nor the additional losses due to magnetizing current. With synchronous motors, there is no difference of speed between air gap rotating magnetic field and rotor.

9 Power factor of induction motor depends on load and speed ,Power factor of a synchronous might be fixed ,usually such motors are huge and therefore their reactive power causes huge losses

10 When ever a synchronous machine( either motor or generator) is being operated at leading power factor(PF), it always shed out its leading Reactive VARs( volta-ampere reactives) for such machine

11 Large synchronous motors have adjustable power factor. They can even have leading power factor. They are often set this way compensate for all the other induction motors. This can effect the efficiency of the motor depending on load. With the system tuned to near unity the entire distribution system benefits.

12 Synchronous motor always rotates with synchronous speed, irrespective of the loading conditions. So, the effective output is not reduced, compared to induction motor. So, more efficiency is observed in this case. Also, the operating power factor is constant in synchronous motors.

13 synchronous machine have separate DC excitation which reduces machine's excitation dependency on main supply, hence better PF. where as IM have no such provisions, hence low PF .

14 Power factor is a number which in very small length tells us about the efficiency of an AC machine like induction motor. As we know, in an inductive load, current lags the voltage by a certain angle. Higher the lag, lesser will be the power factor. ... cosine of the angle between Voltage and Current is called power factor.

15 An over-excited synchronous motor has a leading power factor. This makes it useful for power factor correction of industrial loads. Because the synchronous motor act has a capacitor which is useful in power factor improvement. Hence a synchronous motor is over excited this improves the plant power factor and reduces the reactive current required from the grid.