#  NAME: pirah OKUNTADE shedrack

# MATRIC NUMBER:17/eng06/073

# DEPARTMENT : mechanical engineering

#  ASSIGNMENT 3

1. Given µ= 0.9, , , ,
	1. From continuity equation

q = A.u

where

Because Re < 2000, the flow is laminar

1. Given , G = 0.85, ,

, D = 65mm = 0.065m , L = 95m

 Rate of flow, Q = A.u

 Where

* 1. Centre line velocity =

But,

* 1. Total frictional drag, fD

Where

* 1. Power required to maintain flow

* 1. Velocity gradient at the pipe wall
	2. Velocity and shear stress 60mm from wall

The shear stress can be found as;