**Name: Modilim Tochukwu Adrian**

**Matric No: 17/ENG04/041**

**Department: ELECTRICAL/ELECTRONICS ENGINEERING**

**EEE 382 ASSIGNMENT**

commandwindow

clearvars

clc

close all

format short g

syms t Kp Td Tp x

%Linearized

v= Kp\*(1-exp(-((t-Td)/Tp)))

Adrian=xlsread('1587203818odevbesdata','data1');

t1=Adrian(:,1);

v=Adrian(:,2);

V=round(mdata(900,2),1);

t0=ones(length(v),1);

t=[t0 t1];

[mcoeff, mcoeffint, mrseid, mresidint, manova]=regress(v,t1);

mcoeff

manova

Kp=V

Td=-mcoeff(1)

Tp=mcoeff(2)

figure(1)

plot(t1,v)

hold on

plot(t1,V)

grid on

grid minor

xlabel('Time(min)')

ylabel('Volume(m^3)')

legend('Experimental','Linearized')

%non-linear

ig=[0.1,0.1,0.1,0.1];

modelfun=@(v,t) ig(1)\*(1-exp(-((ig(2)-ig(3))/ig\*4))));

Adr=nlinfit(t1,v,ig,modelfun)

figure(2)

plot(t1,v)

hold on

plot(t1,Adr)

grid on

grid minor

xlabel('Time(min)')

ylabel('Volume(m^3)')

legend('Experimental','Nonlinear')

%comparing

figure(3)

plot(t1,v)

hold on

plot(t1,)

hold on

plot(t1,Adr)

grid minor

grid on

xlabel('Time(min)')

ylabel('Volume(m^3)')

legend('Experimental','Linearlized','Nonlinear')

%SAE

[v,t1]=simplefit\_data1;

net=fitnet(10.'trainscg');

net.performFcn= 'sae';

net= train(net,x,t)

y=net(x)

e=t1-y

perf= sae(net,t,y)

%MAE

y=net(v)

e=t-y

perf= mae(e)

%SSE

[v,t1]=simplefit\_data1;

net= fitnet(10);

net.performFcn= 'sse';

net= train(net,x,t)

y=net(x)

e=t1-y

perf= sse(net,t,y)

.