OKIEMUTE WATERWAY

17/ENG03/056

CIVIL ENGINERRING

ENGINEERING SURVEY II

QUESTION 1

|  |  |
| --- | --- |
| Height of Collimation | Rise and Fall |
| * This method is simple and easy. * Reduction of levels is easy. * Visualization is not necessary regarding the nature of the ground. * There is no check for intermediate sight readings * This method is generally used where more number of readings can be taken with less number of change points for constructional work and profile leveling. | * This method is complicated and is not easy to carry out. * Reduction of levels takes more time. * Visualization is necessary regarding the nature of the ground. * Complete check is there for all readings. * This method is preferable for check levelling where number of change points are more. |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| B.S | I.S | F.S | H OF C | R.L | DISTANCE |
| 0.771 |  |  | 166.771 | 166 | 10 |
| 0.802 |  | 1.52 | 166.053 | 165.251 | 20 |
|  | 2.311 |  |  | 163.742 | 30 |
| 3.580 |  | 1.990 | 167.643 | 164.063 | 40 |
|  | 1.220 |  |  | 166.423 | 50 |
|  | 3.675 |  |  | 163.968 | 60 |
| 2.408 |  | 4.020 | 166.031 | 163.623 | 70 |
|  | 0.339 |  |  | 165.692 | 80 |
| 0.780 |  | 0.157 | 166.654 | 165.874 | 90 |
|  | 1.535 |  |  | 165.119 | 100 |
|  | 1.955 |  |  | 164.699 | 110 |
|  | 2.430 |  |  | 164.224 | 120 |
|  | 2.985 |  |  | 163.669 | 130 |
| 1.155 |  | 3.480 | 164.329 | 163.174 | 140 |
|  | 1.960 |  |  | 162.369 | 150 |
|  | 2.365 |  |  | 161.964 | 160 |
| 0.935 |  | 3.640 | 161.624 | 160.689 | 170 |
|  | 1.045 |  |  | 160.579 | 180 |
|  | 1.630 |  |  | 159.994 | 190 |
|  |  | 2.545 |  | 159.079 | 200 |
| =10.431 |  | =17.352 |  |  |  |

++

Check==R.L at first point-R.L at last point

=6.921=6.921

QUESTION 2

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Chain age(m) | 0 | 30 | 60 | 90 | 120 | 150 | 180 | 210 | 240 | 270 |
| Offset length(m) | 0 | 2.65 | 3.80 | 3.75 | 4.65 | 3.60 | 5.00 | 5.80 | 6.10 | 5.85 |

Using Mid-ordinate rule:

A=hd

h1= =1.325m

h2= =3.225m

h3= =3.775m

h4= =4.2m

h5= =4.125m

h6= =4.3m

h7= =5.4m

h8= =5.9m

h9= =5.925m

38.175m

d=30m

A=

=

A=

Using average ordinate rule

A=

n=9

d=30

41.2m

A=

A=

Using trapezoidal rule

A=

A=

A=

A=

Using Simpson's rule


Note: Last offset was removed because number of offsets were even


Calculating for last offset using trapezoidal rule

A=


Therefore

(b)


* Irregular contours indicate uneven surface.
* Approximately concentric closed contours with decreasing values towards center indicate a pond
* Contour lines generally do not meet or intersect each other. If contour lines are meeting in some portion, it shows existence of a vertical cliff.



* Contour lines with U-shape with convexity towards lower ground indicate ridge.
* Contour lines with V-shaped with convexity towards higher ground indicate valley.



* Contours of different elevations cannot cross each other. If contour lines cross each other, it shows existence of overhanging cliffs or a cave.



* Contour lines cannot end anywhere but close on themselves either within or outside the limit of the map. 