**NAME: Iyamah Osemudiamen Nathaniel**

**MATRIC NO: 17/eng06/048**

**DEPARTMENT: Mechanical Engineering**

**A.**

* **DC power supplies:** Filters are used to eliminate undesired high frequencies (i.e., noise) that are present on AC input lines. Additionally, filters are used on a power supply's output to reduce ripple.
* **Radio Communications:** Filters enable radio receivers to only "see" the desired signal while rejecting all other signals (assuming the other signals have different frequency content).
* **Audio electronics:** A crossover network is a network of filters used to channel low-frequency audio to woofers, mid-range frequencies to midrange speakers, and high-frequency sounds to tweeters.
* Used for Equalizing in Audio Application.
* Used in Receivers for efficient reception of the baseband signals.

**B. Designing a Low-Pass Filter with 0.005Ω resistor and 0.01F capacitor**

**A 100V Amplitude was selected with a frequency of 1Hz for the Sine Wave Source.**

****

**C. Determining the Cut-off frequency**

The cut-off frequency is; F= ½\*(pi\*R\*C)

When R= 0.005Ω and

 C= 0.01F

F= 0.5\*pi\*0.005\*0.01=3189.099 Hz

**D. Design Output**

The transfer function equation for the circuit is given as

(1/RC)/(S + 1/RC)

When R= 0.005Ω and

 C= 0.01F

Transfer Fcn=(1/0.005\*0.01)/(S + (0.005\*0.01))

= (20000)/(s+ 20000)



1. **If two signals of 5 KΩ and 2 KΩ are pass through the filter at different intervals. Discuss your observation**

**When the signal of 5 KΩ is passed through the filter, the following result is obtained:**

The transfer function equation for the circuit is given as

(1/RC)/(S + 1/RC)

When R= 5000Ω and C= 0.01F

Transfer Fcn=(1/5000\*0.01)/(S + (5000\*0.01))= (0.02)/(s+ 0.02)

****

**Observations:** The signal is attenuated to 3.869 ohms

**When the signal of 2K ohms is passed through the filter the following results are obtained:** The transfer function equation for the circuit is given as

(1/RC)/(S + 1/RC)

When R= 2000Ω and

C= 0.01F

Transfer Fcn=(1/2000\*0.01)/(S + (2000\*0.01))= (0.05)/(s+ 0.05)

****

**Observations:** The signal is attenuated to 9.266 ohms