|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NO | DESCRIPTION | UNIT | QUANTITY | RATE | AMOUNT |
| 1 | Supply and laying of a 32in conductor casing suitable for top-hold drilling. For a well operating at a down-hold pressure of 700bar | m | 25 | 2,877 | 500,000 |
| 2 | Supply and laying of big bags of bentonite and barrels of pseudo oil used for producing drilling mud based n specification | Tonnes/barrel | 41 | 3,714 | 227,000 |
| 3 | Supply of natural at a flowrate of 27scfm gases with a pressure of 60 bar at the export line  | scfm | 30 | 3,010 | 800,00 |

UKPAI CHINENYE SHALOM

17/ENG01/028

CHEMICAL ENGINEERING

ENG 384 (JUNE 1ST TEST-2)