17/MHS06/013

MLS 304

Preventive maintenance which include:

Inspection and cleaning

• Clean the surface of the equipment using a natural cleaner or a wet cloth.

• Keep the environment of the working equipment clean.

Testing and adjustment

• Change the fuse when faulty.

• Adjustment of peristaltic pump tube.

• Change of aspiration tube.

• Change the light source lamp.

• Replace invalid filter.

• Daily calibration.

• Lubricate moving parts

• For servicing or repairs, call authorized persons.

Documenting equipment condition

Improvement recommendations