**1a.**

**Rise and Fall :**

* **It is easy to spot errors**
* **It is tedious**
* **It is preffered if there are many intermediate stations**
* **It has more calculations.**

**Height Of Collimation:**

* **It is faster than rise and fall**
* **It is fairly**
* **It is preffered if there are less or no intermediate stations**
* **It is quicker and less of calculation needed.**

****

QUESTION **2a**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Chainage(m) | 0 | 30 | 60 | 90 | 120 | 150 | 180 | 210 | 240 | 270 |
| Offset length(m) | 0 | 2.65 | 3.80 | 3.75 | 4.65 | 3.60 | 5.00 | 5.80 | 6.10 | 5.85 |

Using Mid-ordinate rule:

A=$Σ$hd

h1= $\frac{0+2.65}{2}$=1.325m

h2= $\frac{2.65+3.80}{2}$=3.225m

h3= $\frac{3.80+3.75}{2}$=3.775m

h4= $\frac{3.75+4.65}{2}$=4.2m

h5= $\frac{4.65+3.60}{2}$=4.125m

h6= $\frac{3.60+5.00}{2}$=4.3m

h7= $\frac{5.00+5.80}{2}$=5.4m

h8= $\frac{5.80+6.00}{2}$=5.9m

h9= $\frac{6.00+5.85}{2}$=5.925m

$$Σh=1.325+3.225+3.775+4.2+4.125+4.3+5.4+5.9+5.925$$

$Σh=$38.175m

d=30m

A=$Σhd$

= $38.175×30$

A= $1145.25m^{2}$

Using average ordinate rule

A=$\frac{ndΣO}{n+1}$

n=9

d=30

$$ΣO=0+2.65+3.80+3.75+4.65+3.60+5.00+5.80+6.10+5.85$$

$ΣO=$41.2m

A=$\frac{9×30×41.2}{9+1}$

A=$112.4m^{2}$

Using trapezoidal rule

A=$d(\frac{0\_{1}+0\_{n }}{2}+0\_{2}+0\_{3}+0\_{4}............0\_{n-1})$

$$d=30$$

A=$30(\frac{0+5.85}{2}+2.65+3.80+3.75+4.65+3.60+5.00+5.80+6.10)$

A=$30(38.275)$

A=$1148.25m^{2}$

Using Simpson's rule

$$A=\frac{d }{3 }\left[\left(0\_{1}+0\_{n}\right)+4\left(0\_{2}+0\_{4}+.........0\_{n-1}\right)+2\left(0\_{3}+0\_{5}........0\_{n-1}\right)\right]$$

$$d=30$$

Note: Last offset was removed because number of offsets were even

$$A=\frac{30}{3 }\left[\left(0+6.10\right)+4\left(2.65+3.75+3.60+5,80\right)+2\left(3.80+4.65+5.00\right)\right]$$

$$A=962m^{2}$$

Calculating for last offset using trapezoidal rule

A=$d(\frac{0\_{1}+0\_{n }}{2}+0\_{2}+0\_{3}+0\_{4}............0\_{n-1})$

$$A=30\left[\frac{6.40+5.85}{2}\right]$$

$$A=183.75m^{2}$$

Therefore $ΣA=962+183.75$

$$A=1145.75m^{2}$$

**2b**

NolivALlJlLlJ

contour lines cannot merge or cross one another except in the case of an hanging beam















NOI1<>11J\_J山